###Project Name
project name = ASPEN

###Devie Number
device channel = 3

###planform name
planform name = RTOS

###COM
com bOpen = 0
com base = 1
com count = 1
com baud rate = 38400

path producer = boot\producer_37xx.bin
path nandboot = boot\spiboot_37XX.bin
path nandboot new = Nandboot_37XXL_new.bin
path nand retry = nandretry.bin

producer run addr = 0x30000000

chip type = AK_37XX_C
chip uboot = 1
chip clock = 124
chip power off gpio = 255
chip usb2 = 1
chip pll_frep_change = 0
chip mode = 1
chip update = 0
chip test ram = 0
chip updateself = 0
chip udisk update = 0
chip select number = 1
chip select nand2 = 254
chip select nand3 = 254
chip select gpio = 0
chip gpio_pin = 254

wait time = 30
USB PID = e101
USB VID = 04d6
burned mode = 1
burned gpio = 1, 254, 1, 0, 255
burned rtc = 1, 1

cmdline support = 1
cmdline address = 0x0
cmdline data = 

ram type = 1
ram size = 16
ram row = 13
ram column = 9
ram bank = 4

mac start high = 60:01:02
mac start low = 03:04:05
mac end high = 60:01:02
mac end low = FF:FF:FF
mac addr flag = 1
fore write mac addr = 1

serial start num = REALAND0000000000020180130000001
serial addr flag = 0
fore write serial addr = 1
otp serial flag = 0
otp serial num = 0020180130000001

online make image = 0

moduleburn DownloadMode = 0
moduleburn bDownloadFLS = 1
moduleburn bDownloadEEP = 1
moduleburn baudrate = 921600
moduleburn gpio_dtr = 85
moduleburn gpio_module_igt = 109
moduleburn gpio_module_reset = 87
moduleburn path_fls = LCG2.fls
moduleburn path_eep = LCG2.eep

fs reserver block = 64
fs nonfs reserve size = 4

partition count = 5
	partition1 = C, 0, 0, 0, 20
	partition2 = D, 0, 0, 0, 20
	partition3 = A, 0, 0, 0, 10
	partition4 = E, 0, 0, 0, 10
	partition5 = B, 1, 0, 0, 4000

volume lable count = 5
volume lable1 =  
volume lable2 =  
volume lable3 =  
volume lable4 =  
volume lable5 =  

download_to_udisk count = 0

download_to_nand count = 4
download_to_nand1 = 0, Sword_355.bin, 0x30000000, BIOS, 0, 0
download_to_nand2 = 0, AkResData.Bin, 0x30200000, RES, 0, 0
download_to_nand3 = 0, LangCodepage_spi.bin, 0x30200000, LANG, 0, 0
download_to_nand4 = 0, DynamicFont4_16_spi.bin, 0x30200000, FONT, 0, 0

download_to_mtd count = 0

nand supported count = 0

spinand supported count = 0

sflash supported count = 3
sflash 1 = 0x1740c8, 8388608,  256, 256, 65536, 10000000, 0x0, 0x0, 25Q64BSIG, 0
sflash 2 = 0x1720c2, 8388608,  256, 256, 65536, 10000000, 0x0, 0x0, 未知, 0
sflash 3 = 0x1740ef, 8388608,  256, 256, 65536, 10000000, 0x0, 0x0, , 0
