## 6.6 Real-time Monitoring

Monitor the statuses and real-time events of doors under the access control panels in the system in real-time, including normal events and exceptional events (including alarm events).

1. Monitoring all:

The system will, by default, show the monitoring of all doors under the control panels within the current user¡¯s access level. The user can monitor one (or more) door(s) by [Area], [Control panel] or [Door].

Remote Opening/Closing: involved in control on single door and all doors. In single-door control, move the cursor to the door icon, click [Remote opening/closing] in the displayed dialog box. In all current doors control, directly click [Close all current doors] in the main interface to fulfill the operation.

For remote unlock, you can self-define the open time duration in the displayed dialog box (the default unlock duration is 15s); or you can select [Enable Intraday Normal Open Time Zone], and then the intraday normal-open time segment set by the system becomes effective; furthermore, you can set the door status to normal-open, and then the door is open without time restriction (that is, the door is 24-hour open).

If you want to close the door, you must select [Disable Intraday Normal Open Time Zone] firstly to prevent door opening from other normal-open time segment enabling, and then select [Remote Closing] to fulfill the operation.

? Note: If the operations of remote opening/closing always return failure, please check the current list of devices. If there are too many offline devices, you need to check the network to ensure the operation proceed normally.

Cancel the alarm: Once an alarming door is displayed on the interface, you can hear the alarm sound. Alarm cancellation is involved in control on single door and all doors. In single-door control, move the cursor to the icon of the door, and then click [Cancel the alarm] in the displayed dialog box. In all-door control, directly click [Cancel all alarms]. If the alarm is cancelled successfully, the alarm sound is disappeared automatically.

? Note: If the system reports that alarm cancellation fails, check whether too many devices in the device list are disconnected. If yes, check the network status; otherwise, you cannot operate on the system.

Upon Door Status Monitoring, if the number of doors on the current interface <=64, the system will, by default, show the doors in pictures to monitor door statuses. Once the number exceeds 64, the system will automatically list the doors.

When putting the cursor on a door, it will show relevant parameters and operations: device, door number, door name, door status, relay status and alarm type, remote opening, remote closing and cancel alarm.

Icons in different colors represent statuses as follows:

Icon |  |  |  |  |  |
Status | Device banned | Door Offline | Door sensor unset Relay closed /Without relay status | Door sensor unset Relay opened /Without relay status | Online status : Door closed Relay closed /Without relay status | Online status : Door closed Relay opened /Without relay status
Icon |  |  |  |  |  |
Status | Online status : Door opened Relay closed /Without relay status | Online status : Door opened Relay opened /Without relay status | Door opened alarming Relay closed | Door opened alarming Relay opened | Door opening timeout Relay closed /Without relay status | Door opening timeout Relay opened /Without relay status
Icon |  |  |  |  |  |
Status | Door closed alarming Relay closed /Without relay status | Door closed alarming Relay opened /Without relay status | Door sensor unset Door alarming Relay closed | Door sensor unset Door alarming Relay opened |  |

? Note: Without relay status, denotes that the current firmware does not support "detect relay status" function.

Personnel photo display:

If the Real-Time Monitoring is involved in a person, the monitor displays the personal photo (if no photo is registered, No photo displays). The event name, time and name are displayed on the personal photo.

Event monitoring:

The system automatically acquires monitored device event records, including normal access control events and exceptional access control events (including alarm events). Alarm events appear in red. Exceptional events excluding alarm events appear in orange. Normal events appear in green.

On the current event monitoring interface, the recent records are on the top, enabling the user to see without dragging the scrollbar. Meanwhile, the interface will show up to some 50 records.

2. Alarm Events:

Actually, Alarm Events indicates monitoring the alarm status of the doors. If a door sends an alarm, and the page will always display the alarm status. A door may have multiple alarm states, which represent different alarm types. In the descending severity order, the alarm types are as follows: tamper-resistant alarm > intimidation alarm (password + fingerprint) > intimidation password or finger print alarm > unexpected opening alarm > opening timeout alarm.

Note: The alarm type is displayed only when the firmware version of the device supports alarm type description.

Notification: Enter the recipient e-mail address (separate multiple addresses with semicolon (;)), and then send all door alarm records in the alarm event monitoring list to the recipient.

Cancel alarm: Select the door in alarm status, and then click [Cancel alarm] to cancel the alarm status.

Cancel all alarms: Click [Cancel all alarms] to cancel the alarm status of all doors.

The alarm event monitoring list is shown below:

3. Electro-Map

Before using the electro-map, user needs to add the map in the system first. After success adding, user can add door, camera, zoom-in, zoom-out the map (and the door on the map), etc. If the user changes the position of icon or the map, click [Save Position] to save the current position, then the user can view the setting at the next time access.

Add Map and Delete Map: User can add or delete the map as needed.

Edit Map: User can change the map name, change map or change the area it belongs to.

Adjust map (includes door): User can add a door or a camera on the map, or delete an exist one (right click the door icon or camera, and select [Remove Door]or [camera]), or adjust the map or position of the door or camera icon (by drag the door or camera icon), adjust the size of the map (click [Zoom in] or [Zoom out]or click on [Full Screen] ).

Real-time door status monitoring: Except to display the electro-map, the system can view the real-time event monitoring (same data source with door status monitoring, include alarm sound, etc.).

Door operation: Move the mouse icon to the door position, the system will automatically filter the operation according to the door status and display them on the popup menu. User can remote open or close the door, cancel alarm, and etc.

Camera Operation: Double-click the [camera icon], can be real-time preview video monitor screen.

? Note: Camera function only supports 5.2.20 or above version.

User right control:

(1) In adding process, user needs to select the belonging area for map. The area set here is relevant to the user management rights, that is, the user can only view or manage the map under his rights. If the user modify the belonging area of a map, all door on that map will be cleared, and need to add again.

(2) When the administrator add a new user, he can manage the user operation rights by role setting, such as the operation of [Save door position], [Zoom in], [Zoom out], etc.

? Notes:

(1) In map modification, the user can select to modify the map name but not the path, only need to cancel the tick before [Modify Path].

(2) The system supports to add multi door at the same time. After door adding, user needs to set the door position on the map, and click [Save] after setting.

(3) In door position modifying, especially zoom in the map, the margin of upward and leftward should be smaller than 5 pixels. The system will prompt error if the margin smaller than this value.

(4) The system recommend adding map size under 1120 pixels * 380 pixels. If the multi clients access the same server, the display effect will be differed according to the resolution of screen and the setting of the browser.

Appendixes: Real-Time Event Description (the fingerprint events are only available for 5.2.20 and above version):

1. Normal Events:

Normal Punch Open: In [Card Only] verification mode, the person has open door permission punch the card and trigger this normal event of open the door.

Press Fingerprint Open: In [Fingerprint Only] or [Card plus Fingerprint] verification mode, the person has the open permission, press the fingerprint at the valid time period, and the door is opened, and triggers the normal event.

Card plus Fingerprint Open: In [Card plus Fingerprint] verification mode, the person has the open permission, punch the card and press the fingerprint at the valid time period, and the door is opened, and triggers the normal event.

Exit button Open: User press the exit button to open the door within the door valid time zone, and trigger this normal event.

Trigger the exit button (locked): indicates the normal event triggered by pressing the exit button when the exit button is locked

Punch during Normal Open Time Zone: At the normally open period (set to normally open period of a single door or the door open period after the first card normally open), or through the remote normal open operation, the person has open door permission punch the effective card at the opened door to trigger this normal events.

Press Fingerprint during Normal Open Time Zone: At the normally open period (set to normally open period of a single door or the door open period after the first card normally open), or through the remote normal open operation, the person has open door permission press the effective fingerprint at the opened door to trigger this normal events.

First Card Normal Open (Punch Card): In [Card Only] verification mode, the person has first card normally open permission, punch card at the setting first card normally open period but the door is not opened, and trigger the normal event.

First Card Normal Open (Press Fingerprint): In [Fingerprint Only] or [Card plus Fingerprint] verification mode, the person has first card normally open permission, press the fingerprint at the setting first card normally open period but the door is not opened, and triggers the normal event.

First Card Normal Open (Card plus Fingerprint): In [Card plus Fingerprint] verification mode, the person has first card normally open permission, punch the card and press the fingerprint at the setting first card normally open period but the door is not opened, and triggers the normal event.

Normal Open Time Zone Over: After the setting normal open time zone, the door will close automatically. The normal open time zone include the normal open time zone in door setting and the selected normal open time zone in first card setting.

Remote Normal Opening: Set the door state to normal open in the remote opening operation, and trigger this normal event.

Cancel Normal Open: Punch the valid card or use remote opening function to cancel the current door normal open state, and triggers this event.

Disable Intraday Normal Open Time Zone: In door normal open state, punch the effective card for five times near to the card reader (must be the same user), or select [Disable Intraday Normal Open Time Zone] in remote closing operation, and trigger this normal event.

Enable Intraday Normal Open Time Zone: If the intraday door normal open time zone is disabled, punch the effective card for five times near to the card reader (must be the same user), or select [Enable Intraday Normal Open Time Zone] in remote opening operation, and trigger this normal event.

Multi-Card Open (Punching Card): In [Card Only] verification mode, multi-card combination can be used to open the door. After the last piece of card verified, the system trigger this normal event.

Multi-Card Open (Press Fingerprint): In [Fingerprint Only] or [Card plus Fingerprint] verification mode, multi-card combination can be used to open the door. After the last fingerprint verified, the system trigger this normal event.

Multi-Card Open (Card plus Fingerprint): In [Card plus Fingerprint] verification mode, multi-card combination can be used to open the door. After the last card plus fingerprint verified, the system trigger this normal event.

Multi-Card Open (Press Fingerprint): In [Card Only] verification mode, multi-card combination can be used to open the door. After the last fingerprint verified, the system trigger this normal event.

Multi-Card Open (Card plus Fingerprint): In [Card Only] verification mode, multi-card combination can be used to open the door. After the last card plus fingerprint verified, the system trigger this normal event.

Emergency Password Open: The password (also known as the super password) set for the current door can be used for door open. It will trigger this normal event after the emergency password verified.

Open during Normal Open Time Zone: If the current door is set a normally open period, the door will open automatically after the setting start time, and trigger this normal event.

Linkage Event Triggered: After the system linkage configuration take effect, trigger this normal event.

Cancel Alarm: When the user cancel the alarm of the corresponding door, and the operation is success, trigger this normal event.

Remote Opening: When the user opens a door from remote and the operation is successful, it will trigger this normal event.

Remote Closing: When the user close a door from remote and the operation is successful, it will trigger this normal event.

Open Auxiliary Output: In linkage action setting, if the user select Auxiliary Output for Output Point Address, select Open for Action Type, it will trigger this normal event when the linkage setting is take effect.

Close Auxiliary Output: In linkage action setting, if the user select Auxiliary Output for Output Point Address, select Open for Action Type, it will trigger this normal event when the linkage setting is take effect. And if the user closes the opened auxiliary output through the [Close Auxiliary Output] operation in [Door Setting], trigger this normal event too.

Door Opened Correctly: When the door sensor detects that the door has been properly opened, triggering this normal event.

Door Closed Correctly: When the door sensor detects that the door has been properly closed, triggering this normal event.

Auxiliary Input Disconnected: When the auxiliary input point disconnected, trigger this normal event.

Auxiliary Input Shorted: When the auxiliary input point short circuit, trigger this normal event.

Device Start: When the device start trigger this normal event, and this event can not display on the real-time monitor, but you can check it in the event report.

2. Abnormal Events

Too Short Punch Interval: When the interval between two card punching is less than the set time interval, trigger this abnormal event.

Too Short Fingerprint Pressing Interval: When the interval between two card punching is less than the set time interval, trigger this abnormal event.

Door Inactive Time Zone (Punch Card): In [Card Only] verification mode, the user has the door open permission, punch card but not at the door effective period of time, and trigger this abnormal event.

Door Inactive Time Zone (Press Fingerprint): The user has the door open permission, press the fingerprint but not at the door effective period of time, and trigger this abnormal event.

Door Inactive Time Zone (Exit Button): The user has the door open permission, punch card but not at the access effective period of time, and trigger this abnormal event.

Illegal Time Zone: The user with the permission of opening the current door, punches the card during the invalid time zone, and triggers this abnormal event.

Access Denied: The registered card without the access permission of the current door, punch to open the door, trigger this abnormal event.

Anti-Passback: When the anti-pass back setting of the system takes effect, triggers this abnormal event.

Interlock: When the interlocking rules of the system take effect, trigger this abnormal event.

Multi-Card Authentication (Punching Card): Use multi-card combination to open the door, the card verification before the last one (whether verified or not), trigger this normal event.

Multi-Card Authentication (Press Fingerprint): Use multi-card combination to open the door, the fingerprint verification before the last one (whether verified or not), trigger this normal event.

Multi-Card Authentication (Punching Card): Use multi-card combination to open the door, the card verification before the last one (whether verified or not), trigger this normal event.

Multi-Card Authentication (Press Fingerprint): In [Fingerprint Only] or [Card plus Fingerprint] verification mode, use multi-card combination to open the door, the fingerprint verification before the last one (whether verified or not), trigger this normal event.

Unregistered Card: Refers to the current card is not registered in the system, trigger this abnormal event.

Unregistered Fingerprint: Refers to the current fingerprint is not registered or it is registered but not synchronized with the system, trigger this abnormal event.

Opening Timeout: The door sensor detect that it is expired the delay time after opened, if not close the door, trigger this abnormal event.

Card Expired: The person with the door access permission, punch card to open the door after the effective time of the access control, can not be verified and will trigger this abnormal event.

Fingerprint Expired: The person with the door access permission, press fingerprint to open the door after the effective time of the access control, can not be verified and will trigger this abnormal event.

Password Error: Use card plus password, duress password or emergency password to open the door, trigger this event if the password is wrong.

Failed to Close during Normal Open Time Zone: The current door is in normal open state, but the user can not close the door through [Remote Closing] operation, and trigger this abnormal event.

3. Emergency Events

Duress Password Open: Use the duress password of current door verified and triggered alarm event.

Opened Accidentally: Except all the normal events (normal events such as user with door open permission to punch card and open the door, password open door, open the door at normally open period, remote door open, the linkage triggered door open), the door sensor detect the door is opened, that is the door is unexpectedly opened.

Duress Fingerprint Open: Use the duress fingerprint of current door verified and triggered alarm event.

Door-open times out: indicates the alarm event triggered when the locked door is not locked after timeout