## 7.2 Video Linkage Settings

Bind the video channel and the door for which association needs to be set. You can set the binding between the door reader and the video channel on the door edit page. For details, see 6.3.1 Door Management. Alternatively, bind the door reader and the video channel in [Channel Management]. The operation flow of binding the video channel and the door reader on the [Channel Management] page is as follows:

¡ý

The method of setting video association is the same as that of setting door controller association. Set the trigger condition and video input position, and select relevant options on the association setup page. For details, see 6.3.6 Linkage Setting.