## 6.8 Access Control Parameter Settings

Set some of the software functions, including [Set the time for obtaining new events], [Configure real time monitoring], [Set retry interval after the device is offline], [Configure the Mailbox Server]. After the settings are completed, manually restart the software service through the service console; otherwise, the setting will not become effective.

Set the time for obtaining new events:

Select interval for new events:

Set the record download interval upon the setting becomes effective.

Set the time for obtaining new events:

The system downloads the record at the specified time points automatically.

Configure real time monitoring:

If select [Yes], when the software service is enabled, the software automatically acquires the real-time event record from the device whether the browser is open for real-time monitoring or not, and the software saves the record in the database.

If select [No], only when the browser is open and monitors in real time, the software can acquire the real-time event record from the device.

Set retry interval after the device is offline:

The software attempts to reconnect the disconnected devices at a default interval of 60s. If you want to reconnect the devices faster, you can advisably modify the value. The smaller value occupies more resources of the server.

Configure the Mailbox Server:

Set the information of the mail server sending e-mails. The e-mail addresses receiving e-mails should be set in linkage settings.

? Note: In mail server setting, the e-mail address and mail server (SMTP) must have the same domain name. For example, if the e-mail address is test@gmail.com, the mail server address must be smtp.gmail.com.