Help Center -> Access Control System Management -> Door settings

## Door Settings

Currently the system supports the connection and control of up to 50 access control panels.
The access control system is primarily for the management of personnel forbidden and admission. For security, a company will set personnel admission time zones, forbidden time zones and combinations of time zones. For door opening verification, First-Card Normal Open, Multi-Card Opening, anti-passback, linkage, and interlock can be set to enhance security. This system can provide real-time monitoring of doors and output of exception, access control events and access level reports.

### Door Management

Click [Access control] - [Door configuration], and by default it will access [Door management] interface, showing the list of all control panels. When unfolded, it can show all doors under the control of the control panel. Upon first entry into the access interface or successful query, if currently the system has access control panels or the query result is not null, by default it will unfold the doors of the first access control panel. Click corresponding button for relevant parameter setting.
Door management operations include: control panel management and door management.
1. Control panel operation
For communication between the system and the device, data uploading, configuration downloading, device and system parameters shall be set. The user can see access control panels within his levels in the current system, and can edit the devices here. If the user needs to add or delete devices, operate in device management.
Control panel management includes: Modify IP address, Close auxiliary output, disable, Enable, Modify communication password, Synchronize time, Upload event record, Upgrade firmware, and Get event entries.
(1) Device profile:
Select device, click [Edit] under “Related operation”. For Related details, see Device Maintenance.
(2) Modify IP address:
Select device, and click [Modify IP address] to show the modification interface. Enter new IP address, gateway, and subnet mask. Click [OK] to save settings and quit. This function is same as [Modify IP address function] in Access Control Device. The difference is when searching control panels, the devices have not been added into the system, while the current [Modify device IP address] is regarding added devices.
(3) Disable/Enable :
Select device, click [Disable/ Enable] to stop/ start using the device. When the device’s communication with the system is interrupted or the device fails, the device may automatically appear in disabled status. At this time, after adjusting Internet or device, click [Enable device] to reconnect the device and restore device communication.
Note: If the current device is in enabled status and the connection is not successful, and the user conducts enable operation, the system will immediately reconnect the device.
(4) Modify communication password:
Enter the same new password for twice, and click [OK] to modify the communication password.
Note: The communication password can not contain space, it is recommended to use a combination of numbers and letters. The communication password setting can improve the device security, it is recommended to set communication password for each device.
(5) Synchronize time:
Synchronize device time with current server time.
(6) Get event entries:
Get event records in the device into the system.
Two options is provided for this operation, Get New Entries and Get All Entries.
Get New Entries: The system only get the new event entries after the last time event entries getting, and record them into the database, the repeated entries will not rewrite again.
Get All Entries: The system will get all of the event entries again, the repeated entries will not rewrite again.
When the network status is normal and the communication status between the system and the device is normal, the system will acquire event records in the device in real-time and save them into system database. However, when the network is interrupted or communication is interrupted for some reasons, and the event records in the device have not been uploaded into the system in real-time, this operation can be used to manually acquire event records in the device. In addition, the system, by default, will automatically acquire event records in the device at 00:00 each day.
Note: The access controller can restore up to 100 thansands of event entries, after the entries exceed this number, the device will automatically delete the oldest restored entries (the default delete number is 10 thansands).
(7) Upgrade firmware
To upgrade firmware in the device, tick the device for which you want to upgrade firmware, click [Upgrade firmware], enter edit interface, click [Browse] to select the firmware upgrade file (named emfw.cfg) provided by us, and click [OK] to start upgrading.
Note: The user shall not upgrade firmware without authorization. Contact the distributor before upgrading firmware, or upgrade it when instructed by the distributor. Unauthorized upgrading may bring problems that affect your normal use.
(8) Change the fingerprint identification threshold
The user can change the fingerprint identification threshold in the device, the scale is 35-70, it is 55 by default. In device adding, the system will get the threshold from device. If the operation succeeds, user can view the threshold in all of the devices. The batch operation is permitted; user can change multi devices meanwhile.
(9) Enable DLST
Select the DLST being set, click [Enable] to enable the DLST.
(10) Disable DLST
Disable the DLST in used.
(11) Get information of personnel
Renew the current number of personnel and fingerprints in the device. And the final value will be displayed on the device list.
(12) Rename auxiliary input
User-defined the auxiliary input name.
(13) Rename auxiliary output
User-defined the auxiliary output name.
2. Door Management:
The device list will show all access control devices. Click the “+” button before the device name to show the door list under a device. When adding device, it will automatically add doors (corresponding device name and door numbers can not be edited) according to the number of doors. Before using the device (including doors), the user must edit door information one by one (or apply current settings to other doors). After editing, they will be sent to the device, which can be used after successful setting.
(1) Door parameter modification:
Select the door to be modified, and click [Edit] under “Related operation” to show the Edit interface;
The fields are as follows:
Device name: It is not editable (need to be edited in 6.2.1 Access control device);
Door number: The system automatically name the numbers of doors according to how many doors of the device (for example, the four doors of a four-door control panel are numbered 1, 2, 3 and 4). The number will be consistent with the door number on the device.
Note: Although by default the number following the underline in the door name is consistent with the door number, but 1/2/3/4 in anti-passback and interlock refers to door serial number rather than the number following the door name, and they have no necessary relation, and the system allows the user to modify the door name, so they can not be confused;
Door name: The default door name is “device name_door number”. The field allows the user to modify as required. Up to 30 characters can be entered;
Door valid time zone, door normal open time zone: By default either is null. Initialized and added access control time zones will be shown for the user to select. Upon door editing, door valid time zone is need to input. Only after setting door valid time zone, the door can be opened and closely normally. We recommend to set door normal open time period within the door valid time zone, only in this situation, the door normal open time zone is valid;
Note: Consecutive punching of a card having access level of the door for 5 times can release the normal open status within one day (including First-Card Normal Open), and close the door immediately.
Lock open duration: Used to control the delay for unlocking after card punching. The unit is second, and the default is 5 seconds. The user can enter a number between 0-254;
Punch interval: The unit is second (range: 0-10 seconds), and the default is 2 seconds;
Door sensor type: NO (door sensor not detected), Normal Open, Normal Close. The default is NO. When editing doors, the user can select the door sensor type to be Normal Open or Normal Close. If Normal Open or Normal Close is selected, it is required to select door status delay and whether close and reverse-lock is required. By default, once door sensor type is set as Normal Open or Normal Close, the default door status delay will be 15s, and by default it will enable close and reverse-lock.
Door status delay: The duration for delayed detection of door sensor after the door is opened. Detection is performed only after the door is opened and the delay duration expired. When the door is not in the “Normally Open” period, and the door is opened, the device will start timing. It will trigger alarm when the delay duration expired, and stop alarm when you close the door. The default door status delay will be 15s. The door status delay should be longer than lock open duration.
Close and reverse-lock: Set locking or not after door closing. Tick it for lock after door closing.
Verify mode: Supports Only Card and Password Plus Card verify modes. The default is Only Card. When Password Plus Card mode is selected, make sure the door uses a reader with keyboard;
Wiegand Card Format: Select the reader can identify the card format;
Request to Exit: When the exit button triggered the door is not open after the exit is without unlock;
Alarm Delay: The duration for delayed detection of request to exit after the exit is without unlock;
Duress password, emergency password (named super password): Upon duress, use duress password (used with legally card) to open the door. Upon emergency, the user can use emergency password to open the door. When opening the door with duress password (used with legally card), it will alarm. Emergency password allows normal door opening.
Duress password opening (used with legally card): When Only Card verify mode is used, you need press [ESC] first, and then press the setting password plus [OK] button, finally swipe your card, the door open and trigger the alarm. When Password Plus Card verify mode is used, please swipe your card first, then press the password number plus [OK] button (same to normal door open in card plus password verify mode), the door open and trigger the alarm.
Emergency password opening: The password must be a number not exceeding 8 digits (integer). The door can be opened just by entering the password. Please press [ESC] every time before entering password, and then press OK to execute.
When using duress password or emergency password, the interval for entering each number shall not exceed 10 seconds, and these two number should not be the same.
Apply the setting to all doors of the current control panel: Click to apply to all doors of the current control panel;
Apply the setting to all doors of all control panels: Click to apply to all doors of all control panels within the current user’s level;
Reader: Rename the reader;
After parameter editing, click [OK] to save and quit.