Help Center -> Device Management -> Communication command details

## Communication command details (only used for attendance)

The list shows the details of communication commands between the device and the system, namely, description of commands sent by server.
Times of processing: The system command is automatically sent after unsuccessful execution. The default maximum number is 3 times.
Processing flag: Indicate the command sent successfully or not, doesn’t indicate the execution state.
Device executing command progress: Indicate the progress of server execute the command, 100% means execution successfully.