## 9.3 Visitor Management

Choose Visitor System ¡ú Visitor Manage, as shown in the following figure.

Visitor Manage covers Enroll visitor and Exit visitor. Click Enroll visitor when a visitor comes to have a visit and click Exit visitor when the visitor exits. Both card registration and on-site snapshot capture are supported during registration.

Choose Visitor System ¡ú Visitor Manage ¡ú Enroll visitor to access the entry registration page, as shown in the following figure.

Choose Visitor System ¡ú Visitor Manage ¡ú Exit visitor to access the exit registration page, as shown in the following figure.

The visitor system is highly integrated with the access control system and elevator control system. Door access rights must be granted to visitors. To grant rights to visitors, grant some rights to visitors in the rights group of the access control system or elevator control system, and then grant specific rights to the visitors in Enroll visitor, as shown in the following figure.

?Note: Complete the following settings before using the USB camera-based capture function: Right-click Capture in the capture frame and choose Global Settings from the shortcut menu. On the Storage tab page, click Local Storage Settings by Site to add a website address. Add 127.0.0.1 if the computer is a server, and add the IP address of the server such as 192.168.8.12 if the computer is a client. Set the website to be allowed on the Camera and Mic and Playback tab pages. The settings need to be completed only once as long as history records of the browser are not deleted. If the camera does not capture any pictures, check whether the settings are correct and whether the camera indicator is on, close and then open the browser again.

?Note: The camera can be loaded and invoked only by one page at a time.